{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"merged":[[0,0,1,4],[16,2,16,4]],"flags":["formulas_cached_only"]}
["六号楼夹层装修的项目及要求（用于配网终端产品）"]
[]
["序号","名称","单位","数量","备注"]
[1,"矿棉板吊顶","㎡",560]
[2,"防静电地坪漆","㎡",560,"1  整体打磨清扫。\n2  涂刷环氧底漆。\n3  批刮环氧砂浆，打磨清扫。\n4  批刮环氧腻子。\n5  贴导电铜箔。\n6  涂刷导电底漆两遍。\n7  施工防静电自流平。"]
[3,"消防喷淋改造","个",66]
[4,"双开木门","樘",4]
[5,"单开木门","樘",1]
[6,"门禁","套",2,"海康威视等一线品牌，刷脸，密码"]
[7,"5p立式空调","台",3,"美的5p"]
[8,"轻质隔墙200","㎡",98]
[9,"墙面腻子两遍乳胶漆","㎡",668]
[10,"水电开槽布线人工费+材料费","㎡",530]
[11,"LED平板灯","个",36,"白光100w。国内一线品牌。\n一个大区隔配一个开关"]
[12,"PZ箱（含开关及插座）","个",9,"配三相4P开关1只，2P开关1只，2P漏保开关1只，三相4脚叉1只，单相3脚叉2只（含老化间2个）。\n用国产一线品牌的配件。"]
[13,"风淋室","台",1,"参数见附表"]
[14,"其他要求","1、所有材料全包。\n2、工期1个月内完成。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}